SECOND HARMONIC GENERATION IN PHOTONIC CRYSTAL FIBER

$∬\_{}^{}E$sh\*Ef dxdy

ESH IS ONE OUTPUT

EF IS ONE OUTPT