**The structure is three dimensional**

**Input of the Structure**

Cladding

Core 1

Core 2

**Port Definition:**

**Port1** includes Core1, Core2 and Cladding. Port Type is numerical and excitation on.

**Port2** includes Core1, Core2 and Cladding. Port Type is numerical and should be off because I would like to make excitation through Core1 and see how the coupling ratio between those is.

**Port3** includes Core1`s output, Core2´s output and Cladding. Port Type is numerical and excitation off.

**Port4** includes Core1`s output, Core2´s output and Cladding. Port Type is numerical and excitation off

Which number should I enter for “search mode around” ncore or clad?